

EMU-2 Meter Monitor getting connected with Smart Meter

**Smart Meter Configuration**


1.Follow the steps below to configure the Smart Meter via optical cable.



2. In step 6, the MAC ID and Install code should be registered.




Once registration finished, then click HAN registration, the device info should be like this picture. The HAN key is generated from Install code.




3. Then Turn HAN join on.

**On EMU monitor side**

Basically, you do not need to do anything, just start the power and it will search for the meter automatically and then join. If the screen shows **connection lost, rejoining meter,** then you need to Hard Reset the device.

Hard Reset Steps:


Once it is connected, the monitor should show the synchronous time.



**RAVEn USB Sticker**

For RAVEn USB sticker connect to smart meter, follow the same steps above to configure smart meter. Then, plug in the sticker to PC, and open **personal meter reader** to see if it connects.

There is a LED on the sticker displaying its connection status.



If the connection failed, the problem is probably due to **hard reset**. Similarly, open **personal meter reader, and find hard reset option, then hard reset your device.**

